**Unit #1602**

**2006 Komatsu PC 1800-6 Excavator**

**Serial # KMTPC081J02011071**

Location – Oil Sand Operation, Fort McMurray, AB, Canada

Area – Support Shop Yard

SMU – 44,000

**Component Hours (SMU)**

Engine – Front – 3,650 Rear – 6,835

Hyd. Pump All four at 3,672

Swing:

Transmission – Front – 3,672 Rear – 7,680

Motor - Front – 2,057 Rear – 7,680

Pumps - #1 – 3,672 #2 – 3,672

Propel:

Transmission – LH – 15,891 RH – 15,891

Motor – LH – Front – 29,840 RH – Front – 6,020

LH – Rear – 29,840 RH – Rear – 2,057

Side Frame – LH – 30,741 RH – 30,741

Track – LH – 10,475 RH – 10,475

Bucket – 1,438

Cylinder – Boom – LH – 1,831 RH – 9,684

Stick – LH – 0 RH – 1,831

Curl – LH – 9,062 RH – 6,049

Unit comes complete with a 2-stage wet and dry fire suppression system

**See the following 3 pictures of the excavator taken in March 2018**





