

Quotation 21-170

FK-14392 25 Barrel Flare Knockout

48” Diameter x 10’ Flare Knockout Vessel on Saddles

6” 150# RFWN Inlet/Gas Outlet

18” Round Access Manway

External Float Chamber with (2) 2” NPT Nozzles

2” NPT PSV Nozzle

Penberthy Sightglass & Valves

2” NPT Drain with Valve

PI & TI

12’6” x 5’6” x 12” High Containment

12’6” x 5’6” x 6” Structural Steel Skid with Roll Ends