|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CNRL Business District**  (e.g. NE Gas, St. Albert, Bonnyville, Edson) | **Grande Prairie** | | | **MT #** (from attached blank MT) | | |  | | | | |
| **Date of Insp.** | | | 8/31/2011 | | | | |
| **Prov. Reg.#**  (e.g. A#. RAE#, C#) | A3106404 | | | **Location**  (Field Name) | | | HAMBURG PLANT | | | | |
| **Equipment Type** (e.g. treater, separator, scrubber) | RICH GLYCOL FLASH DRUM | | | **LSD** | | | 12-29-096-11W6 | | | | |
| **Previous LSD** | | |  | | | | |
| **Tag/Equip. #**  (e.g. V-101) | V-2400 | | | **Comp./Unit #**  (e.g. 1408) | | |  | | | | |
| Vessel Status: | In Service X | Not In Service | | **Job #** | | |  | | | | |
| Fabricator | I.P CONSTRUCTORS | Serial # | | 95-1677 | | | MAWP/Temp | | | 150 PSI  200 F | |
| CRN# | M8555.2 | Shell Mat’l | | SA-516-70N | | | Shell Thick. | | | 0.375 | |
| Corr. All. | 0.0625 | Head Mat’l | | SA-516-70N | | | Head Thick. | | | 0.337 | |
| Diameter | 2 FT | Length |  | Height | 8 FT | | RT |  | | HT |  |
| Year Built | 1995 | Next Insp. | |  | | | Insp. Type | | |  | |
| Service | SWEET | Manway | | N | | | Coating | | |  | |
| **PSV #.** |  | | | | | | | | | | |
| **Mfg.** |  | **Serial #** | |  | | **Set Pressure** | | |  | | |
| **Type/Model** |  | **Capacity** | |  | | **Size** | | |  | | |
| **Date of Service** |  | **Next Service** | |  | | **Service Co.** | | |  | | |

**Notes: PSV 10 FT OFF GROUND Report #**

**Completed by: Don Burren Contact Number: 403-304-4951**